{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Instructions","Wiring Diagram","Zeroing Form"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Wiring Diagram","index":1,"n_rows":6,"n_cols":7,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Wiring your X-Carve for a Touch Plate"]
[]
[]
[null,null,null,null,null,null,"Adding Touch Plate is an easy upgrade and will allow you to zero your machine in all 3 axis very accurately."]
[null,null,null,null,null,null,"Below are the steps to follow:"]

{"sheet":"Zeroing Form","index":2,"n_rows":20,"n_cols":16,"rows_kept":20,"cut":false,"hidden":false,"merged":[[1,0,1,18],[17,10,17,13],[18,10,18,13],[5,2,5,6],[19,3,19,4],[17,3,17,6],[8,1,8,2],[7,3,7,6],[8,3,8,6],[6,3,6,6],[16,10,16,13],[3,2,3,4],[4,2,4,4],[6,1,6,2],[7,1,7,2]]}
[]
["Enter your data in the green boxes only."]
[]
[null,null,"Bit Diameter ",null,null,null,"Inches"]
[null,null,"Touch Plate Thickness",null,null,null,"Inches"]
[null,null,"Copy and Past codes from this column"]
[null,"Z Axis G-Code",null,"G38.2 Z-.5 F1;G92 Z0.5;G0 Z0.25"]
[null,"X Axis G-Code",null,"G38.2 X-.5 F1;G92 X0.125"]
[null,"Y Axis G-Code",null,"G38.2 Y-.5 F1;G92 Y0.125"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"G38.2 Z-.5 F1;G92 Z",null,{"$f":"F5","v":0},";","G0 Z",0.25]
[null,null,null,null,null,null,null,null,null,null,"G38.2 X-.5 F1;G92 X",{"$f":"F4/2","v":0}]
[null,null,null,null,null,null,null,null,null,null,"G38.2 Y-.5 F1;G92 Y",{"$f":"F4/2","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(K14,F5,N14,O14,P14)","v":"G38.2 Z-.5 F1;G92 Z;G0 Z0.25"}]
[null,null,null,"Milimeter to Inch Conversion",null,null,null,null,null,null,{"$f":"CONCATENATE(K15,L15)","v":"G38.2 X-.5 F1;G92 X0"}]
[null,null,null,"Millimeters",null,0,"Enter mm here only",null,null,null,{"$f":"CONCATENATE(K16,L16)","v":"G38.2 Y-.5 F1;G92 Y0"}]
[null,null,null,"Inches",null,{"$f":"F19*0.03937008","v":0},"Do not enter data in the yellow box… It contains a foumula to make the conversion"]